Reliability Types

Control how and when with packet priority and reliability types enum PacketPriority { HIGH_PRIORITY, MEDIUM_PRIORITY, LOW_PRIORITY, NUMBER_OF_PRIORITIES }; PacketPriority is simple. High priority packets go out before medium priority packets and medium priority packets go out before low priority packets do. Originally I raised the priority of packets that took a long time to get out, but in practice this would disrupt games in progress as unimportant data to new connections (such as the map data) would get in the way of the game data. enum PacketReliability { UNRELIABLE, UNRELIABLE_SEQUENCED, RELIABLE, RELIABLE_ORDERED, RELIABLE_SEQUENCED }; Unreliable Unreliable packets are sent by straight UDP. They may arrive out of order, or not at all. This is best for data that is unimportant, or data that you send very frequently so even if some packets are missed newer packets will compensate. Advantages - These packets don't need to be acknowledged by the network, saving the size of a UDP header in acknowlegement (about 50 bytes or so). The savings can really add up. Disadvantages - No packet ordering, packets may never arrive, these packets are the first to get dropped if the send buffer is full. Unreliable sequenced Unreliable sequenced packets are the same as unreliable packets, except that only the newest packet is ever accepted. Older packets are ignored. Advantages - Same low overhead as unreliable packets, and you don't have to worry about older packets changing your data to old values. Disadvantages - A LOT of packets will be dropped since they may never arrive because of UDP and may be dropped even when they do arrive. These packets are the first to get dropped if the send buffer is full. The last packet sent may never arrive, which can be a problem if you stop sending packets at some particular point. Note that the transmission of one of the three reliable packets types is required for the detection of lost connections. If you never send reliable packets you need to implement lost connection detection manually. Reliable Reliable packets are UDP packets monitored by a reliablilty layer to ensure they arrive at the destination. Advantages - You know the packet will get there. Eventually... Disadvantages - Retransmissions and acknowlegements can add significant bandwidth requirements. Packets may arrive very late if the network is busy. No packet ordering. Reliable ordered Reliable ordered packets are UDP packets monitored by a reliability layer to ensure they arrive at the destination and are ordered at the destination. Advantages - The packet will get there and in the order it was sent. These are by far the easiest to program for because you don't have to worry about strange behavior due to out of order or lost packets. Disadvantages - Retransmissions and acknowlegements can add significant bandwidth requirements. Packets may arrive very late if the network is busy. One late packet can delay many packets that arrived sooner, resulting in significant lag spikes. However, this disadvantage can be mitigated by the clever use of ordering streams . Reliable sequenced Reliable ordered packets are UDP packets monitored by a reliability layer to ensure they arrive at the destination and are sequenced at the destination. Advantages - You get the reliability of UDP packets, the ordering of ordered packets, yet don't have to wait for old packets. More packets will arrive with this method than with the unreliable sequenced method, and they will be distributed more evenly. The most important advantage however is that the latest packet sent will arrive, where with unreliable sequenced the latest packet sent may not arrive. Disadvantages - Wasteful of bandwidth because it uses the overhead of reliable UDP packets to ensure late packets arrive that just get ignored anyway.

See Also

Index Sending Packets